
	s.no 
	Sample lab no
	Mpn 10ml
	Mpn 1ml
	Mpn 0.1ml
	Mpn  result
	Fecal coli form

	1
	24
	0
	0
	0
	0
	-

	2
	25
	3
	0
	1
	11
	+

	3
	28
	1
	0
	0
	2
	-

	4
	43-A
	0
	0
	1
	2
	+

	5
	44-A
	0
	0
	0
	0
	-

	6
	45-C
	0
	0
	0
	0
	_

	7
	12
	0
	1
	3
	7
	+

	8
	10-K
	0
	0
	0
	0
	_

	9
	11-B
	0
	0
	0
	0
	_

	10
	36-D
	1
	0
	0
	2
	-

	11
	56-M
	3
	1
	0
	11
	-

	12
	80-K
	0
	0
	0
	0
	-

	13
	123-T
	3
	0
	0
	8
	+

	14
	100-KK
	0
	0
	0
	0
	-

	15
	45-B
	1
	0
	0
	2
	-

	16
	18-N
	1
	3
	0
	8
	-

	17
	15-S
	3
	1
	0
	11
	+

	18
	28-P
	0
	0
	0
	0
	-

	19
	65-H
	2
	1
	0
	7.6
	+

	20
	32-BD
	0
	0
	0
	0
	-


 Table 3. Shows the bacteriology of bore water collected from different sources. The highest MPN 11 was observed in samples having ID 25, 56-M and 15-S and the lowest 0 was observed in many samples. 



Table 4.Bacteriological analysis of well water 
	s.no
	Sample lab no
	Mpn 10ml
	Mpn1 ml
	Mpn o.1ml
	Mpn result
	Fecal coli form

	1.
	Kk1
	4
	0
	4
	30
	+

	2.
	Kk2
	3
	2
	1
	17
	+

	3.
	Kk3
	0
	0
	0
	0
	-

	4
	Bu 21
	3
	0
	1
	11
	+

	5.
	Dik 54
	1
	0
	0
	2
	-

	6.
	Sw 12
	1
	4
	0
	11
	+

	7.
	Psh 2
	0
	0
	0
	0
	-

	8.
	Psh 3
	1
	2
	4
	15
	+

	9.
	Kt 45
	4
	1
	0
	17
	+

	10.
	Kt 36
	4
	2
	1
	26
	+

	11.
	Kt 47
	0
	0
	0
	0
	-

	12.
	Tk 89
	0
	0
	0
	0
	-

	13.
	Tk 45
	4
	0
	0
	13
	+

	14.
	Lm 20
	3
	1
	0
	11
	+

	15.
	Lm 21
	0
	0
	0
	0
	-

	16.
	Ht 15
	0
	0
	0
	0
	-

	17.
	Ns 10
	4
	1
	1
	21
	+

	18.
	Mat 14
	2
	1
	0
	7
	+

	19.
	Mat 16
	1
	1
	1
	6
	-

	20.
	Mat 17
	3
	0
	1
	11
	-



Table 4. Shows the bacteriology of well water collected from different sources. The highest MPN 30 was observed in sample ID Kk1 followed by kt 36 i-e 26 and , lowest MPN 0 was observed in more than one samples.




Table 5.Bacteriological analysis of bottled water
	s.no
	Sample lab no
	Mpn 10ml
	Mpn 1ml
	Mpn o.1ml
	Mpn result
	Fecal coli form

	1.
	Khyber safe 
	1
	1
	1
	6
	+

	2.
	Saha purified 
	0
	0
	0
	0
	-

	3.
	Aqua safe-03
	2
	0
	0
	5
	+

	4.
	Healthy 
	0
	0
	0
	0
	-

	5.
	Nestle -05
	0
	0
	0
	0
	-

	6.
	Aqua fina-06
	0
	0
	0
	0
	-

	7.
	Kinley clean 
	0
	0
	0
	0
	-

	8.
	Premium water
	1
	0
	0
	2
	+

	9.
	Safa pure-09
	0
	0
	0
	0
	-

	10
	Al saudia-10
	0
	0
	0
	0
	-

	11.
	Ultra pure-11
	0
	0
	0
	0
	-

	12.
	Nestle -A
	0
	0
	0
	0
	-

	13.
	Nestle -B
	0
	0
	1
	2
	+

	14.
	Nestle-c
	0
	0
	0
	0
	-

	15.
	Nestle pure life
	0
	0
	0
	0
	-

	16.
	Pure drinking water (Tb)
	0
	0
	0
	0
	-

	17.
	Sparkletts pure waer
	0
	0
	0
	0
	-

	18.
	Life quality water
	0
	0
	0
	0
	-

	19.
	BSW water
	0
	0
	0
	0
	-

	20.
	Aqua clear
	0
	0
	0
	0
	-



Table 5. Shows the bacteriology of bottled water collected from different sources. The highest MPN 6 was observed in sample ID Khyber safe followed by Aqua safe-03 i-e 5. The lowest MPN 0 was observed in more than one samples.
Table 6.Bacteriological analysis of hotels water samples
	s.no
	Sample lab no
	Mpn 10ml
	Mpn 1ml
	Mpn o.1ml
	Mpn result
	Fecal coli form

	1
	Jalil kababi 1
	4
	3
	1
	33
	+

	2
	Taraskoon psh
	1
	0
	0
	2
	+

	3
	Habibi psh
	0
	1
	1
	4
	+

	4
	Marcopolo psh
	2
	1
	1
	9
	+

	5
	Kashmir hotel kt
	1
	0
	0
	2
	+

	6
	Shinwari hotel kt
	3
	1
	1
	14
	+

	7
	Speen Ghar kt
	4
	0
	0
	13
	+

	8
	Jans hotel kt
	0
	5
	5
	19
	+

	9
	Moon hotel kk       
	1
	1
	1
	6
	+

	10
	Shahid hotel kk
	0
	2
	0
	4
	+

	11
	Super waziristan  kk
	0
	4
	2
	11
	+

	12
	Zam zam hotel kk
	3
	2
	4
	27
	+

	13
	Pak afghan kt
	4
	1
	1
	21
	+

	14
	Zaman hotel bu
	1
	0
	0
	2
	+

	15
	Fish point bu
	2
	5
	5
	32
	+

	16
	Tank hotel dik
	2
	1
	1
	9
	+

	17
	Malik hotel dik
	4
	0
	0
	13
	+

	18
	Zaiqa hotel dik 
	1
	0
	0
	2
	+

	19
	Gul hotel dik
	3
	0
	0
	8
	+

	20
	Babu hotel kt
	2
	5
	4
	29
	+


 Table 6. Shows the bacteriology of Hotels water collected from different sources. The highest MPN 33 was observed in the sample jalil kababi followed by 32 of lab ID Fish point bu and Speen Ghar kt . Lowest MPN 2 was in more than one samples .


Table 6.Bacteriological analysis of tap water
	s.no
	Sample lab no
	Mpn 10ml
	Mpn 1 ml
	Mpno.1ml
	Mpn result
	Fecal coliform

	1
	102 A
	0
	1
	1
	4
	+

	2
	103 B
	4
	0
	1
	17
	+

	3
	104 C
	3
	0
	0
	8
	+

	4
	105 D 
	2
	1
	1
	9
	+

	5
	106 E
	4
	2
	2
	32
	+

	6
	107 F 
	4
	0
	0
	13
	+

	7
	108 G
	3
	1
	1
	14
	+

	8
	109 H
	1
	1
	0
	4
	+

	9
	110 I
	3
	2
	2
	20
	+

	10
	111 J
	1
	0
	0
	2
	+

	11
	112 K
	1
	0
	1
	4
	+

	12
	113 L
	4
	0
	0
	20
	+

	13
	114 M
	1
	0
	0
	3
	+

	14
	115 N
	3
	1
	2
	17
	+

	15
	116 N 
	0
	0
	0
	0
	-

	16
	117 O
	2
	1
	1
	9
	+

	17
	118 D 
	3
	1
	0
	11
	+

	18
	119 C
	2
	2
	1
	12
	+

	19
	120 W
	1
	1
	1
	6
	+

	20
	121 B
	3
	4
	0
	21
	+




Table 7. Shows the bacteriology of Tap water collected from different sources. The highest MPN 32 was observed in the sample 106 E followed by 21 of lab ID 121 B. Lowest 0 was observed in lab ID 116 N. 
Table 7.Chemical analysis of bore water
	s.no
	SO4
	NITRATE mg/l 
	NITRITE mg /l
	CHLORIDE mg/l
	TOTAL SOLUBLE SOILDS

	1
	4.67
	0.99
	0.025
	0
	10

	2
	5.11
	0.60
	0.011
	0
	8

	3
	4.67
	0.09
	0.021
	0
	20

	4
	5.67
	0.28
	0.007
	0
	52

	5
	5.01
	0.19
	0.006
	1.5
	120

	6
	8.01
	0.11
	0.007
	3.1
	45

	7
	6.11
	0.22
	0.015
	0
	02

	8
	3.67
	0.42
	0.036
	0
	230

	9
	8.02
	0.44
	0.027
	5.2
	150

	10
	3.33
	0.31
	0.013
	0
	420

	11
	6.11
	0.24
	0.006
	0
	65

	12
	6.67
	0.20
	0.011
	19
	300

	13
	7.67
	0.23
	0.114
	1.07
	320

	14
	5.01
	0.18
	0.018
	1.9
	105

	15
	8.02
	0.29
	-
	0.88
	400

	16
	6.11
	0.60
	-
	1.23
	165

	17
	3.67
	0.42
	0.013
	1.01
	180

	18
	-
	0.11
	0.021
	1.5
	120

	19
	2.51
	0.15
	0.015
	3.2
	65

	20
	6.23
	-
	0.12
	1.87
	32





Table 8. Shows the chemical analysis of bore water the highest TSS 420 was observed in sample no 10 ,chloride 19 in sample no 12, Nitrite 0.114 in sample no 13, Nitrate 0.99 in sample no 1, SO4 8.02 in sample no 9 & 15. 

Table 9.Chemical analysis of well water
	s.no
	SO4 mg/l
	NITRATE mg/l
	NITRITE mg/l
	CHLORIDE mg/l
	TOTAL SOLUBLE SOLIDS

	1
	0.5
	0.32
	-
	0
	20

	2
	2.5
	0.98
	-
	0
	48

	3
	3.10
	0.52
	0.012
	1.56
	32

	4
	8.52
	0.21
	0.033
	1.23
	56

	5
	1.77
	1.03
	0.05
	0.98
	89

	6
	5.6
	0.336
	0.068
	0.21
	120

	7
	4.25
	0.58
	-
	2.35
	410

	8
	2.3
	0.46
	0.23
	0
	210

	9
	5.23
	0.65
	-
	0
	325

	10
	8.36
	2.11
	0.078
	7.1
	650

	11
	2.33
	0.15
	0.021
	5.6
	21

	12
	9.10
	1.32
	0.045
	2.10
	65

	13
	7.25
	1.21
	0.065
	5.69
	34

	14
	1.5
	0.54
	0.023
	0
	152

	15
	6.41
	0.69
	-
	0
	140

	16
	7.12
	-
	-
	8.36
	65

	17
	3.33
	0.32
	0.015
	3.25
	365

	18
	2.56
	0.89
	0.054
	6.32
	250

	19
	4.98
	0.99
	-
	6.32
	654

	20
	1.77
	0.12
	-
	5.69
	100



Table 8. Shows the chemical analysis of well water the highest TSS 654 was observed in sample no19, chloride 8.36 in sample no 16 , Nitrite 0.23 in sample no 8, Nitrate 2.11 in sample no 10, SO4 9.12 in sample no 12.

Table 10.Chemical analysis of bottled water
	s.no
	SO4 mg/l
	NITRATE mg/l
	NITRITE mg/l
	CHLORIDE mg/l
	TOTAL SOLUBLE SOLIDS

	1
	0.01
	0.23
	0
	14
	20

	2
	0
	0
	0
	2
	12

	3
	0
	0.12
	0.001
	4
	8

	4
	0
	0
	0.021
	3
	15

	5
	0
	0
	0
	0
	0

	6
	0
	0
	0.21
	0
	23

	7
	0
	1
	0.2
	5
	32

	8
	0
	0
	0
	0
	0

	9
	0
	0
	0
	0
	0

	10
	0
	0
	0
	0
	0

	11
	0
	0.36
	0.25
	24
	50

	12
	0
	0
	0
	0
	0

	13
	0
	0
	0
	0
	0

	14
	0
	0
	0
	0
	0

	15
	0
	0
	0
	0
	0

	16
	0
	0
	0
	0
	0

	17
	0
	0
	0
	0
	0

	18
	0
	8
	0.056
	30
	42

	19
	0
	1
	0
	4
	20

	20
	0
	0
	0
	0
	0



Table 10. Shows the chemical analysis of bottled water the highest TSS 50 was observed in sample no11, chloride 30 in sample no 18, Nitrite 0.25 in sample no 11, Nitrate 8 in sample no 18 ., SO4 0.01 in sample no 1.


Table 11.Chemical analysis of hotels water
	S.NO
	SO4 mg/l
	NITRATE mg/l
	NITRITE mg/l
	CHLORIDE mg/l
	TOTAL SOLUBLE SOLIDS

	1
	1.2
	0
	0
	14
	23

	2
	0
	0
	0
	04
	14

	3
	0
	0.12
	0.001
	6
	8

	4
	0
	0
	0.021
	20
	15

	5
	0
	0
	0
	0
	0

	6
	0
	0
	0.21
	5
	23

	7
	0
	1
	0.2
	8
	32

	8
	0
	0
	0
	12
	0

	9
	0
	0
	0
	21
	0

	10
	0
	0
	0
	0
	0

	11
	0
	0.36
	0
	0
	50

	12
	0
	0
	0
	0
	0

	13
	0
	0
	0
	0
	0

	14
	0
	0
	0
	0
	0

	15
	0
	0
	0
	0
	0

	16
	0
	0
	0
	0
	0

	17
	0
	0
	0
	0
	0

	18
	0
	0
	0.56
	3
	42

	19
	0
	1
	0
	52
	20

	20
	0
	0
	0
	0
	0



Table 11. Shows the chemical analysis of hotels water the highest TSS 50 was observed in sample no11, chloride 52 in sample no 19, Nitrite 0.56 in sample no 18 , Nitrate 0.36 in sample no 11., SO4 1.2 in sample no 1. 


Table 12.Chemical analysis of tap water
	s.no
	SO4 mg/l
	NITRATE mg/l
	NITRITE mg/l
	CHLORIDE mg/l
	TOTAL SOLUBLE SOLIDS

	1
	0
	0
	0
	29
	30

	2
	0
	0
	0
	6
	6

	3
	0
	0.12
	0.001
	6
	10

	4
	0
	0
	0.021
	25
	32

	5
	0
	0
	0
	0
	0

	6
	0
	0
	0.21
	0
	5

	7
	0
	1
	0.2
	20
	24

	8
	0
	0
	0
	2
	4

	9
	0
	0
	0
	21
	26

	10
	0
	0
	0
	0
	0

	11
	0
	0.36
	0
	0
	7

	12
	0
	0
	0
	0
	0

	13
	0
	0
	0
	6
	8

	14
	0
	0
	0
	10
	15

	15
	0
	0
	0
	54
	70

	16
	0
	0
	0
	32
	50

	17
	0
	0
	0
	12
	35

	18
	0
	0
	0.56
	45
	55

	19
	0
	1
	0
	21
	40

	20
	0
	0
	0
	0
	0



Table 12. Shows the chemical analysis of tap water the highest TSS 70 was observed in sample no15, chloride 54 in sample no 15 , Nitrite 0.56 in sample no 18, Nitrate 0.36 in sample no 11., SO4 0 to be in all samples.
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